;$$$MyDIT_GenClassCoInst$$$  ; This tag is needed to trigger the device class ;
; Windows Virtual Serial Port Setup File
; Copyright (c) 2006-2011 TCT International Mobile Ltd
; Manufacturer: TCT International Mobile Ltd
;

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %JRDCOMM%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
DriverVer  = 03/14/2011,2.0.6.3
Catalogfile = jrdusbser.cat

[ControlFlags]
ExcludeFromSelect = *

[SourceDisksNames]
  1000 = %JRDSrcDisk%,"",,

[SourceDisksFiles]
  jrdusbser.sys = 1000

[Manufacturer]
%JRDCOMM% = JRDSerialPort, NTia64, NTamd64

[JRDSerialPort]
%JrdDeviceDiag0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_00
%JrdDeviceAGPS0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_01
%JrdDeviceVOICE0017% = JportInstall00, USB\VID_1BBB&PID_0017&MI_02
%JrdDeviceAT0017%    = JportInstall00, USB\VID_1BBB&PID_0017&MI_03
%JrdDeviceDiag0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_00
%JrdDeviceAGPS0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_01
%JrdDeviceVOICE0052% = JportInstall00, USB\VID_1BBB&PID_0052&MI_02
%JrdDeviceAT0052%    = JportInstall00, USB\VID_1BBB&PID_0052&MI_03
%JrdDeviceDiag0000%  = JportInstall00, USB\VID_1BBB&PID_0000&MI_00
%JrdDeviceAT0000%    = JportInstall00, USB\VID_1BBB&PID_0000&MI_01
%JrdDeviceTPST007A%  = JportInstall00, USB\VID_1BBB&PID_007A
%JrdDeviceDiag00B6%  = JportInstall00, USB\VID_1BBB&PID_00B6&MI_00
%JrdDeviceAT00B6%    = JportInstall00, USB\VID_1BBB&PID_00B6&MI_01
%JrdDeviceDiag00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_00
%JrdDeviceAGPS00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_01
%JrdDeviceVOICE00B7% = JportInstall00, USB\VID_1BBB&PID_00B7&MI_02
%JrdDeviceAT00B7%    = JportInstall00, USB\VID_1BBB&PID_00B7&MI_03
%JrdDeviceDiag011E%  = JportInstall00, USB\VID_1BBB&PID_011E&MI_00
%JrdDeviceAT011E%    = JportInstall00, USB\VID_1BBB&PID_011E&MI_01
%JrdDeviceDiag0190%  = JportInstall00, USB\VID_1BBB&PID_0190&MI_00
%JrdDeviceAT0190%    = JportInstall00, USB\VID_1BBB&PID_0190&MI_01
%JrdDeviceDiag0196%  = JportInstall00, USB\VID_1BBB&PID_0196&MI_02
%JrdDeviceDiag0197%  = JportInstall00, USB\VID_1BBB&PID_0197&MI_00
%JrdDeviceDiag01AA%  = JportInstall00, USB\VID_1BBB&PID_01AA&MI_03
%JrdDeviceDiag0203%  = JportInstall00, USB\VID_1BBB&PID_0203&MI_00
%JrdDeviceDiag0204%  = JportInstall00, USB\VID_1BBB&PID_0204&MI_00

[JRDSerialPort.NTia64]
%JrdDeviceDiag0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_00
%JrdDeviceAGPS0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_01
%JrdDeviceVOICE0017% = JportInstall00, USB\VID_1BBB&PID_0017&MI_02
%JrdDeviceAT0017%    = JportInstall00, USB\VID_1BBB&PID_0017&MI_03
%JrdDeviceDiag0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_00
%JrdDeviceAGPS0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_01
%JrdDeviceVOICE0052% = JportInstall00, USB\VID_1BBB&PID_0052&MI_02
%JrdDeviceAT0052%    = JportInstall00, USB\VID_1BBB&PID_0052&MI_03
%JrdDeviceDiag0000%  = JportInstall00, USB\VID_1BBB&PID_0000&MI_00
%JrdDeviceAT0000%    = JportInstall00, USB\VID_1BBB&PID_0000&MI_01
%JrdDeviceTPST007A%  = JportInstall00, USB\VID_1BBB&PID_007A
%JrdDeviceDiag00B6%  = JportInstall00, USB\VID_1BBB&PID_00B6&MI_00
%JrdDeviceAT00B6%    = JportInstall00, USB\VID_1BBB&PID_00B6&MI_01
%JrdDeviceDiag00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_00
%JrdDeviceAGPS00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_01
%JrdDeviceVOICE00B7% = JportInstall00, USB\VID_1BBB&PID_00B7&MI_02
%JrdDeviceAT00B7%    = JportInstall00, USB\VID_1BBB&PID_00B7&MI_03
%JrdDeviceDiag011E%  = JportInstall00, USB\VID_1BBB&PID_011E&MI_00
%JrdDeviceAT011E%    = JportInstall00, USB\VID_1BBB&PID_011E&MI_01
%JrdDeviceDiag0190%  = JportInstall00, USB\VID_1BBB&PID_0190&MI_00
%JrdDeviceAT0190%    = JportInstall00, USB\VID_1BBB&PID_0190&MI_01
%JrdDeviceDiag0196%  = JportInstall00, USB\VID_1BBB&PID_0196&MI_02
%JrdDeviceDiag0197%  = JportInstall00, USB\VID_1BBB&PID_0197&MI_00
%JrdDeviceDiag01AA%  = JportInstall00, USB\VID_1BBB&PID_01AA&MI_03
%JrdDeviceDiag0203%  = JportInstall00, USB\VID_1BBB&PID_0203&MI_00
%JrdDeviceDiag0204%  = JportInstall00, USB\VID_1BBB&PID_0204&MI_00

[JRDSerialPort.NTamd64]
%JrdDeviceDiag0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_00
%JrdDeviceAGPS0017%  = JportInstall00, USB\VID_1BBB&PID_0017&MI_01
%JrdDeviceVOICE0017% = JportInstall00, USB\VID_1BBB&PID_0017&MI_02
%JrdDeviceAT0017%    = JportInstall00, USB\VID_1BBB&PID_0017&MI_03
%JrdDeviceDiag0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_00
%JrdDeviceAGPS0052%  = JportInstall00, USB\VID_1BBB&PID_0052&MI_01
%JrdDeviceVOICE0052% = JportInstall00, USB\VID_1BBB&PID_0052&MI_02
%JrdDeviceAT0052%    = JportInstall00, USB\VID_1BBB&PID_0052&MI_03
%JrdDeviceDiag0000%  = JportInstall00, USB\VID_1BBB&PID_0000&MI_00
%JrdDeviceAT0000%    = JportInstall00, USB\VID_1BBB&PID_0000&MI_01
%JrdDeviceTPST007A%  = JportInstall00, USB\VID_1BBB&PID_007A
%JrdDeviceDiag00B6%  = JportInstall00, USB\VID_1BBB&PID_00B6&MI_00
%JrdDeviceAT00B6%    = JportInstall00, USB\VID_1BBB&PID_00B6&MI_01
%JrdDeviceDiag00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_00
%JrdDeviceAGPS00B7%  = JportInstall00, USB\VID_1BBB&PID_00B7&MI_01
%JrdDeviceVOICE00B7% = JportInstall00, USB\VID_1BBB&PID_00B7&MI_02
%JrdDeviceAT00B7%    = JportInstall00, USB\VID_1BBB&PID_00B7&MI_03
%JrdDeviceDiag011E%  = JportInstall00, USB\VID_1BBB&PID_011E&MI_00
%JrdDeviceAT011E%    = JportInstall00, USB\VID_1BBB&PID_011E&MI_01
%JrdDeviceDiag0190%  = JportInstall00, USB\VID_1BBB&PID_0190&MI_00
%JrdDeviceAT0190%    = JportInstall00, USB\VID_1BBB&PID_0190&MI_01
%JrdDeviceDiag0196%  = JportInstall00, USB\VID_1BBB&PID_0196&MI_02
%JrdDeviceDiag0197%  = JportInstall00, USB\VID_1BBB&PID_0197&MI_00
%JrdDeviceDiag01AA%  = JportInstall00, USB\VID_1BBB&PID_01AA&MI_03
%JrdDeviceDiag0203%  = JportInstall00, USB\VID_1BBB&PID_0203&MI_00
%JrdDeviceDiag0204%  = JportInstall00, USB\VID_1BBB&PID_0204&MI_00

[JportInstall00.NT]
CopyFiles=JRDUsbDriverFiles
AddReg = All00, AddReg

[JRDUsbDriverFiles]
jrdusbser.sys

[DestinationDirs]
DefaultDestDir = 12

[JportInstall00.NT.Services]
AddService=jrdusbser,  0x00000002, JRD_USBSerialService

[All00]
HKR,,NTMPDriver,,jrdusbser.sys

[AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"
HKLM,SYSTEM\CurrentControlSet\Control\UsbFlags,IgnoreHWSerNum1BBB011E,1,1
HKLM,SYSTEM\CurrentControlSet\Control\UsbFlags,IgnoreHWSerNum1BBB007A,1,1
HKLM,SYSTEM\CurrentControlSet\Control\UsbFlags,IgnoreHWSerNum1BBB0197,1,1

[JRD_USBSerialService]
DisplayName   = %JRDUSBSER%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\jrdusbser.sys

[Strings]
JRDUSBSER = "Mobile Connector Device for Legacy Serial Communication2"
JRDSrcDisk = "Modem Interface Driver Disk"
JRDCOMM = "hspa Modem"
JrdDeviceDiag0017 = "Application1 port"
JrdDeviceAGPS0017 = "Application2 port"
JrdDeviceVOICE0017= "Application3 port"
JrdDeviceAT0017   = "Application4 port"
JrdDeviceDiag0052 = "Alcatel HSPA 3G DIAG"
JrdDeviceAGPS0052 = "Alcatel HSPA 3G NMEA"
JrdDeviceVOICE0052= "Alcatel HSPA 3G Voice"
JrdDeviceAT0052   = "Alcatel HSPA 3G Mobile"
JrdDeviceDiag0000 = "Application1 interface"
JrdDeviceAT0000   = "Application2 interface"
JrdDeviceTPST007A = "TPST Upgrading Port"
JrdDeviceDiag00B7 = "Application1 Port"
JrdDeviceAGPS00B7 = "Application2 Port"
JrdDeviceVOICE00B7= "Application3 Port"
JrdDeviceAT00B7   = "Application4 Port"
JrdDeviceDiag00B6 = "Application1 Interface"
JrdDeviceAT00B6   = "Application2 Interface"
JrdDeviceDiag011E = "Application1 interface"
JrdDeviceAT011E   = "Application2 interface"
JrdDeviceDiag0190 = "Application1 interface"
JrdDeviceAT0190   = "Application2 interface"
JrdDeviceDiag0196 = "Alcatel Diagnostic port"
JrdDeviceDiag0197 = "Alcatel Diagnostic port"
JrdDeviceDiag01AA = "Alcatel Diagnostic port"
JrdDeviceDiag0203 = "Alcatel Diagnostic port"
JrdDeviceDiag0204 = "Alcatel Diagnostic port"